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Sizewell C Notice to Mariners No 33 of 2026
Pipe-pull Works adjacent to Sizewell C Harbour
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SZC Harbour Master
Date: 19/08/2026  
Any further enquiries regarding this Notice to Mariners should be directed to the ICCB project manager – Tony Lock at: t.lock@iccb.ie
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EA1N & EA2 Windfarm Pipe Pull Works

Mariners are advised that:

Between August 20™-22"¢ 2026 Pipe Pull work is scheduled on the EATN and EA2 wind farm export cable pre-
installation works off the coast at Thorpeness, just to the south of the Sizewell C Harbour Authority area. This work
is complex and will involve several vessels and the Jack-Up-Barge Haven Seachallenger located in position:

Latitude Longitude
52°10.976’N | 001°38.639'E
A floating pipeline approximately 1800m in length will be towed into the area by the tug THOR with the multicat
OCEAN SUPPLIER managing the tail of the tow and with two guard vessels in attendance, one to the north and
one to the south of the pipeline.

The installation work will focus around the Jack-Up Barge (JUB) and the GPS 301 Pontoon, secured to a four-point
mooring approximately 50 metres to seaward of the JUB, but during the initial phase of the pull-in the floating pipe
will extend a significant distance from the JUB in an arc extending in a NE to SE direction according to the state of

the tide. The below illustration highlights the approximate area and for the safety of all concerned, vessels are
requested not to enter this zone.

Lagens
[ s 02 e o
3 o e 04 o o

e

o]

ot

FT T

nrE

W8 Tsoswn

e

Thorpe P

Ness

i
eness [¢

-

ifshore Wind

it TWO -HOD P End Locaten &
o e Jone o

Fig. 1. Exclusion Zone

In addition to the tug THOR and the multicat OCEAN SUPPLIER the tugs CT PRENTON and HANS, together with
the multicats PAUL D and SOPHIA D will be assisting with managing the pipe. Mariners are requested to exercise

additional vigilance and an effective lookout when approaching the area during this period of increased marine
activity.
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Allvessels engaged in these works will abide by and display all shapes and lights required by the COLREGS.
Vessels will monitor VHF Channels 12 and 16.
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